**NOVEXCOMM CLOCK/ VOLTAGE/ TEMPERATURE METER PANEL**

****

**1U RACK PANEL WITH 2 METERS & “ON THE AIR” IN RED BACKLIGHT**

**UTC/ LOCAL TIME, DC VOLTS & DEGREES CELSIUS DISPLAY**

**ALL 3 CYCLE DISPLAY OR FIX ON ONE OF THEM AS NEEDED**

**ORDER YOURS CUSTOM BUILT WITH YOUR CALL SIGN CENTERED**

**SETTING INSTRUCTIONS: MODE ON LEFT, SET ON RIGHT BUTTON**

**Mode setting button:**  
**Short press to select the clock, seconds, voltage, temperature display mode for one specific display OR:  
Long press to show “ALL”, Enter the time temperature voltage alternating display mode, interval of 5 seconds with a Short press to EXIT**

**SET Time setting button:  
Short press to adjust the hours, minutes (flashing), Short press again to exit  
Short press the "Mode setting button", the clock starts running (full colon symbol flashes once per second)**

**Red = + DC source from 7-20 VDC, Black = Negative**

**Green = + lead to attach to your battery/ power supply for DC metering**

**Long black lead is the thermistor; put one on the rig PA final amplifier and one in open-air to watch the temperature differential from ambient**

****

**Visit [www.Novexcomm.com](http://www.Novexcomm.com) or call 310.534.4456 to order yours TODAY!**